Changes from Volta-Interface Rev 01

* Increased board dimensions to 90x26mm
* Increased clearances around the rotary encoder
* Shifted position of binding posts, encoder and switches
* Reduced backplane drill size for binding posts
* Adjusted display connector position and increased clearance
* Added soft-start capacitor to the reset line on the display
* Changed U2 to STM32G031F8P6 to increase program flash