Changes from Volta-Motherboard Rev 01

* Adjusted the front facing board outline to support larger front panel CCA
* Changed U10 to STM32G031F8P6 to increase program flash
* Changed U15 to MCP47CMB22 to improve the DC precision and resolution of the current limit setpoint
* ILIM now comes from a dedicated DAC
* MCP6L2T replaced with TLV272 due to product availability
* Current sense resistor value changed to 0.33 Ohm
* Differential amplifier gain increased to 10V/V